/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2022-09-30
 *
 * @attention
 *
 *  Copyright (C) 2022-2024 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example shows how to use the TMR peripheral to generate a One pulse Mode
after a falling edge of an external signal is received in Timer Input pin.
The TIM3 waveform can be displayed using an oscilloscope.

&par Directory contents

  - TMR/TMR_SinglePulse/apm32f035_int.c     Interrupt handlers
  - TMR/TMR_SinglePulse/Source/main.c              Main program

&par IDE environment

  - MDK-ARM V5.36
  - EWARM V8.50.5.26295
  - ECLIPSE V4.24

&par Hardware and Software environment

  - This example runs on APM32F035 MINI Devices.