/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2025-11-01
 *
 * @attention
 *
 *  Copyright (C) 2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

The program demonstrates how to use polling to send and receive data using USART.
In this example, USART1 and USART2 exchange data with each other. After each
transmission, data verification is performed. If the data transmission from 
USART1 to USART2 is successful, LED1 will turn on. Similarly, if the data 
transmission from USART2 to USART1 is successful, LED2 will turn on.

&par Hardware Description

USART1_TX(PD15) ----> USART2_RX(PC12)
USART1_RX(PD12) ----> USART2_TX(PD0)

  - USART1 and USART2 configured as follow:
  - BaudRate = 115200
  - Word Length = USART_WordLength_8b
  - Stop Bit = USART_StopBits_1
  - Parity = USART_Parity_No
  - Hardware flow control disabled (RTS and CTS signals)
  - Receive and transmit enabled

&par Directory contents
  - USART/USART_Polling/Source/main.c                              Main program implementing the test
  - USART/USART_Polling/Source/g32r4xx_int.c                       Interrupt handlers

&par IDE environment

  - MDK-ARM V5.43
  - EWARM V9.60.2.5599

&par Hardware and Software environment

  - This example runs on G32R430 TINY Devices.