/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2025-11-01
 *
 * @attention
 *
 *  Copyright (C) 2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This is a example that communicates using SPI1 in BISS-C mode.

Connection Details
MB5U Emulator pin connections to the G32R430 TINY board:
┌────────────────────┬────────────────────────┐
│ MB5U Emulator Pin  │ TINY Board Connection  │
├────────────────────┼────────────────────────┤
│ Pin 4              │ C_A                    │
│ Pin 3              │ C_B                    │
│ Pin 8              │ D_A                    │
│ Pin 7              │ D_B                    │
│ Pin 9              │ GND                    │
└────────────────────┴────────────────────────┘

Test Procedure
1. Connect the G32R430 TINY board and MB5U emulator to the computer via USB.
2. Download the BS project to the G32R430 TINY board.
3. Configure the upper computer with the following parameters:
   - MasterClockFrequencySensor: 2.0 MHz.
   - Frame Repetition Rate Sensor: 62.5 us.
   - Frame Repetition Rate Register: 62.5 us.
   - Select BiSS-C mode.
   - Configure CRC Polynomial to 0x43.
   - Set SCD Length to 50 bits.

&par Hardware Description

&par Directory contents

  - SPI/SPI_Biss-C_Slave/Source/main.c                             Main program implementing the test
  - SPI/SPI_Biss-C_Slave/Source/g32r4xx_int.c                      Interrupt handlers

&par IDE environment

  - MDK-ARM V5.42
  - EWARM V9.60.2.5599

&par Hardware and Software environment

  - This example runs on G32R430 TINY Devices.