/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2025-11-01
 *
 * @attention
 *
 *  Copyright (C) 2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This snippet configures essential G32R430 MCU settings by writing values to the Option Bytes at 0x1FFF0000.
It sets read protection levels, toggles software watchdogs, manages write protection, and defines the boot address..

&par Hardware Description

&par Directory contents

  - FLASH/FLASH_OPT/Source/main.c                                  Main program implementing the test
  - FLASH/FLASH_OPT/Source/g32r4xx_int.c                           Interrupt handlers

&par IDE environment

  - MDK-ARM V5.43
  - EWARM V9.60.2.5599

&par Hardware and Software environment

  - This example runs on G32R430 TINY Devices.