/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.3
 *
 * @date        2025-05-31
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */


&par Example Description

This example describes how to use FreeRTOS create multiple tasks.

Usart test task : USART1 received data from upper computer and then keep sending
the received data to upper computer.

Led toggle task : The LED2 and LED3 is configured to toggle constantly


&par Software Description

Please install the following dependencies in the directory where the installation package resides beforehand.
  - Middlewares/FreeRTOS/FreeRTOSv202012.00-LTS.exe   FreeRTOS Software Components


&par Hardware Description

USART1_TX(PD5)
USART1_RX(PD6)


&par Directory contents

  - FreeRTOS/Source/apm32f00x_int.c             Interrupt handlers
  - FreeRTOS/Source/main.c                      Main program
  - FreeRTOS/Include/FreeRTOSConfig.h           FreeRTOS configure functions


&par Hardware and Software environment
  - This example runs on APM32F003 MINI Devices.


&par IDE environment

MDK-ARM V5.36
EWARM V8.50.5.26295
Eclipse V2022-06（4.24.0）
