/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2025-05-31
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */


&par Example Description

This example provides how to use ADC's Difference mode.
In this example, ADC will calculate the difference between two channels,
and output the value to upper computer by Uart1.


&par Hardware Description

J2 and J3 Should be shorted.
using ADC_CH1(PC5), ADC_CH2(PC6).
using LED2(PB5).
USART1 TX(PD6)


&par Directory contents

  - USART/ADC_DiffMode/Source/apm32f00x_int.c      Interrupt handlers
  - USART/ADC_DiffMode/Source/main.c               Main program


&par Hardware and Software environment

  - This example runs on APM32F003 MINI Devices.


&par IDE environment

MDK-ARM V5.36
EWARM V8.50.5.26295
Eclipse V2022-06（4.24.0）
