/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.3
 *
 * @date        2025-05-31
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */


&par Example Description

This example describes how to use RTX5 create multiple tasks.

Usart test task : USART1 and USART2 send or received data to each other. Verification will occur after transmission,
if send and received data pass, LED3 will be on all the time.
if send and received data fault, LED3 will be off all the time.
if send or received data fault, LED3 will be constantly flickered alternately.

Led toggle task : The LED2 is configured to toggle constantly


&par Software Description

Please unzip the following dependencies in the directory where the package resides beforehand.
  - Middlewares/RTX5/CMSIS_5-develop.zip        RTX5 Software Components


&par Hardware Description

USART1_TX(PD5)  ----> USART2_RX(PD2)
USART1_RX(PD6)  ----> USART2_TX(PD3)


&par Directory contents

  - RTOS/RTX/Source/apm32f00x_int.c     Interrupt handlers
  - RTOS/RTX/Source/main.c              Main program


&par Hardware and Software environment

  - This example runs on APM32F003 MINI Devices.


&par IDE environment

MDK-ARM V5.36
EWARM V8.50.5.26295
Eclipse V2022-06（4.24.0）
