/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.3
 *
 * @date        2025-05-31
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */


&par Example Description

This example describes how to use WUPT peripheral.


&par Hardware Description

J2 and J3 Should be shorted.
using LED2(PB5).
using LED3(PB4).
using KEY1(PD6).


&par Software Description

Each time the key1 be pressed, the MCU will toggle some while than enter STOP mode
and OFF all LED. When the MCU be awakened, the LED2 will OFF and LED3 will ON.


&par Directory contents

  - WUPT/WUPT/Source/apm32f00x_int.c    Interrupt handlers
  - WUPT/WUPT/Source/main.c             Main program


&par Hardware and Software environment

  - This example runs on APM32F003 MINI Devices.


&par IDE environment

MDK-ARM V5.36
EWARM V8.50.5.26295
Eclipse V2022-06（4.24.0）
