/**
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2025-06-01
 *
 * @attention
 *
 *  Copyright (C) 2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example describes how to use the ADC1 to convert the internal temperature sensor's voltage
applied to the ADC1_Channel 16.
And Calculate the temperature according to the formula as follow:
T = (V - 0.7782)/0.0024 + 28;

The converted voltage and temperature are displayed on serial assistant through USART1.

note:
        According to actual test data of multiple bathes of chips,
        V28 is adopted instead of V25 for this example. And 0.7782v is the voltage for 28 degrees celsius

&par Hardware Description

The UART0 is configured as follows:
    - TX:PA7, RX:PA8
    - BaudRate = 115200 baud
    - Word Length = 8 Bits
    - One Stop Bit
    - No parity
    - Hardware flow control disabled (RTS and CTS signals)
    - Receive and transmit enabled

&par Directory contents

  - ADC/ADC_TemperatureSensor/Source/main.c                   Main program
  - ADC/ADC_TemperatureSensor/Source/g32m3101_int.c         Interrupt handlers

&par IDE environment

  - MDK-ARM V5.36
  - EWARM V8.50.5.26295
  - ECLIPSE-EMB V4.24.0

&par Hardware and Software environment

  - This example runs on G32M3101 EVAL Devices.
