/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2025-11-01
 *
 * @attention
 *
 *  Copyright (C) 2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example demonstrates a simple embedded system initialization sequence for GPIO, DAC,
and comparator peripherals.

- The program initializes an analog input pin for the comparator (PD12) and configures the DAC
to output a fixed voltage (1.65V).
- After initialization, the program enters an infinite loop, where it continuously reads the
comparator output to determine whether the analog input voltage is higher or lower than the DAC
output voltage, and toggles LEDs accordingly.

&par Hardware Description

using COMP1+(PD12)

USART2_TX(PD0)
USART2_RX(PC12)

  - USART2 configured as follow:
  - BaudRate = 115200
  - Word Length = USART_WordLength_8b
  - Stop Bit = USART_StopBits_1
  - Parity = USART_Parity_No
  - Hardware flow control disabled (RTS and CTS signals)
  - Receive and transmit enabled

&par Directory contents

  - COMP/COMP_CompareGpioVsDacInt_OutputGpio/Source/main.c         Main program implementing the test
  - COMP/COMP_CompareGpioVsDacInt_OutputGpio/Source/g32r4xx_int.c  Interrupt handlers

&par IDE environment

  - MDK-ARM V5.40
  - EWARM V9.60.2.5599
  - Eclipse V4.35.0 RC1 &  clang version 19.1.1

&par Hardware and Software environment

  - This example runs on G32R430 TINY Devices.